Drill Press Mounted Centering Ring Cutter

Designed and Drawn by Jim Horner

horner@hpl.hp.com

10–24 x 3/8” (Qnty: 4)

6–32 x 1/4” (Qnty: 8) to hold

blade in place

1/4” bolt. Cut head off with

Dremel tool or hacksaw

3/8” od washers

(Qnty: 4)

Drill and tap

top holes for

10–24 threads

#1 1 X–acto type blade

Make two blade holders from aluminum angle stock

Drill and tap side holes

for 6–32 threads

Use 3/16” drill and dremel tool

to cut slots in 3/32” x 3/4” by

6” aluminum stock

Drill Press Mounted Centering Ring Cutter

Designed and Drawn by Jim Horner

horner@hpl.hp.com