This is nasm.info, produced by Makeinfo version 3.12h from nasmdoc.texi.

INFO-DIR-SECTION Programming
START-INFO-DIR-ENTRY
* NASM: (nasm).                The Netwide Assembler for x86.
END-INFO-DIR-ENTRY


   This file documents NASM, the Netwide Assembler: an assembler
targetting the Intel x86 series of processors, with portable source.

   Copyright 2003 The NASM Development Team

   All rights reserved. This document is redistributable under the
licence given in the file "COPYING" distributed in the NASM archive.


File: nasm.info,  Node: Section B.4.14,  Next: Section B.4.15,  Prev: Section B.4.13,  Up: Section B.4

B.4.14. `BOUND': Check Array Index against Bounds
-------------------------------------------------

     BOUND reg16,mem               ; o16 62 /r            [186]
     BOUND reg32,mem               ; o32 62 /r            [386]

   `BOUND' expects its second operand to point to an area of memory
containing two signed values of the same size as its first operand (i.e.
two words for the 16-bit form; two doublewords for the 32-bit form). It
performs two signed comparisons: if the value in the register passed as
its first operand is less than the first of the in-memory values, or is
greater than or equal to the second, it throws a `BR' exception.
Otherwise, it does nothing.


File: nasm.info,  Node: Section B.4.15,  Next: Section B.4.16,  Prev: Section B.4.14,  Up: Section B.4

B.4.15. `BSF', `BSR': Bit Scan
------------------------------

     BSF reg16,r/m16               ; o16 0F BC /r         [386]
     BSF reg32,r/m32               ; o32 0F BC /r         [386]

     BSR reg16,r/m16               ; o16 0F BD /r         [386]
     BSR reg32,r/m32               ; o32 0F BD /r         [386]

   * `BSF' searches for the least significant set bit in its source
     (second) operand, and if it finds one, stores the index in its
     destination (first) operand. If no set bit is found, the contents
     of the destination operand are undefined. If the source operand is
     zero, the zero flag is set.

   * `BSR' performs the same function, but searches from the top
     instead, so it finds the most significant set bit.

   Bit indices are from 0 (least significant) to 15 or 31 (most
significant).  The destination operand can only be a register. The
source operand can be a register or a memory location.


File: nasm.info,  Node: Section B.4.16,  Next: Section B.4.17,  Prev: Section B.4.15,  Up: Section B.4

B.4.16. `BSWAP': Byte Swap
--------------------------

     BSWAP reg32                   ; o32 0F C8+r          [486]

   `BSWAP' swaps the order of the four bytes of a 32-bit register: bits
0-7 exchange places with bits 24-31, and bits 8-15 swap with bits 16-23.
There is no explicit 16-bit equivalent: to byte-swap `AX', `BX', `CX'
or `DX', `XCHG' can be used. When `BSWAP' is used with a 16-bit
register, the result is undefined.


File: nasm.info,  Node: Section B.4.17,  Next: Section B.4.18,  Prev: Section B.4.16,  Up: Section B.4

B.4.17. `BT', `BTC', `BTR', `BTS': Bit Test
-------------------------------------------

     BT r/m16,reg16                ; o16 0F A3 /r         [386]
     BT r/m32,reg32                ; o32 0F A3 /r         [386]
     BT r/m16,imm8                 ; o16 0F BA /4 ib      [386]
     BT r/m32,imm8                 ; o32 0F BA /4 ib      [386]

     BTC r/m16,reg16               ; o16 0F BB /r         [386]
     BTC r/m32,reg32               ; o32 0F BB /r         [386]
     BTC r/m16,imm8                ; o16 0F BA /7 ib      [386]
     BTC r/m32,imm8                ; o32 0F BA /7 ib      [386]

     BTR r/m16,reg16               ; o16 0F B3 /r         [386]
     BTR r/m32,reg32               ; o32 0F B3 /r         [386]
     BTR r/m16,imm8                ; o16 0F BA /6 ib      [386]
     BTR r/m32,imm8                ; o32 0F BA /6 ib      [386]

     BTS r/m16,reg16               ; o16 0F AB /r         [386]
     BTS r/m32,reg32               ; o32 0F AB /r         [386]
     BTS r/m16,imm                 ; o16 0F BA /5 ib      [386]
     BTS r/m32,imm                 ; o32 0F BA /5 ib      [386]

   These instructions all test one bit of their first operand, whose
index is given by the second operand, and store the value of that bit
into the carry flag. Bit indices are from 0 (least significant) to 15
or 31 (most significant).

   In addition to storing the original value of the bit into the carry
flag, `BTR' also resets (clears) the bit in the operand itself. `BTS'
sets the bit, and `BTC' complements the bit. `BT' does not modify its
operands.

   The destination can be a register or a memory location. The source
can be a register or an immediate value.

   If the destination operand is a register, the bit offset should be
in the range 0-15 (for 16-bit operands) or 0-31 (for 32-bit operands).
An immediate value outside these ranges will be taken modulo 16/32 by
the processor.

   If the destination operand is a memory location, then an immediate
bit offset follows the same rules as for a register. If the bit offset
is in a register, then it can be anything within the signed range of
the register used (ie, for a 32-bit operand, it can be (-2^31) to (2^31
- 1)


File: nasm.info,  Node: Section B.4.18,  Next: Section B.4.19,  Prev: Section B.4.17,  Up: Section B.4

B.4.18. `CALL': Call Subroutine
-------------------------------

     CALL imm                      ; E8 rw/rd             [8086]
     CALL imm:imm16                ; o16 9A iw iw         [8086]
     CALL imm:imm32                ; o32 9A id iw         [386]
     CALL FAR mem16                ; o16 FF /3            [8086]
     CALL FAR mem32                ; o32 FF /3            [386]
     CALL r/m16                    ; o16 FF /2            [8086]
     CALL r/m32                    ; o32 FF /2            [386]

   `CALL' calls a subroutine, by means of pushing the current
instruction pointer (`IP') and optionally `CS' as well on the stack,
and then jumping to a given address.

   `CS' is pushed as well as `IP' if and only if the call is a far
call, i.e. a destination segment address is specified in the
instruction.  The forms involving two colon-separated arguments are far
calls; so are the `CALL FAR mem' forms.

   The immediate near call takes one of two forms (`call imm16/imm32',
determined by the current segment size limit. For 16-bit operands, you
would use `CALL 0x1234', and for 32-bit operands you would use `CALL
0x12345678'. The value passed as an operand is a relative offset.

   You can choose between the two immediate far call forms (`CALL
imm:imm') by the use of the `WORD' and `DWORD' keywords: `CALL WORD
0x1234:0x5678') or `CALL DWORD 0x1234:0x56789abc'.

   The `CALL FAR mem' forms execute a far call by loading the
destination address out of memory. The address loaded consists of 16 or
32 bits of offset (depending on the operand size), and 16 bits of
segment. The operand size may be overridden using `CALL WORD FAR mem' or
`CALL DWORD FAR mem'.

   The `CALL r/m' forms execute a near call (within the same segment),
loading the destination address out of memory or out of a register. The
keyword `NEAR' may be specified, for clarity, in these forms, but is
not necessary. Again, operand size can be overridden using `CALL WORD
mem' or `CALL DWORD mem'.

   As a convenience, NASM does not require you to call a far procedure
symbol by coding the cumbersome `CALL SEG routine:routine', but instead
allows the easier synonym `CALL FAR routine'.

   The `CALL r/m' forms given above are near calls; NASM will accept the
`NEAR' keyword (e.g. `CALL NEAR [address]'), even though it is not
strictly necessary.


File: nasm.info,  Node: Section B.4.19,  Next: Section B.4.20,  Prev: Section B.4.18,  Up: Section B.4

B.4.19. `CBW', `CWD', `CDQ', `CWDE': Sign Extensions
----------------------------------------------------

     CBW                           ; o16 98               [8086]
     CWDE                          ; o32 98               [386]

     CWD                           ; o16 99               [8086]
     CDQ                           ; o32 99               [386]

   All these instructions sign-extend a short value into a longer one,
by replicating the top bit of the original value to fill the extended
one.

   `CBW' extends `AL' into `AX' by repeating the top bit of `AL' in
every bit of `AH'. `CWDE' extends `AX' into `EAX'. `CWD' extends `AX'
into `DX:AX' by repeating the top bit of `AX' throughout `DX', and
`CDQ' extends `EAX' into `EDX:EAX'.


File: nasm.info,  Node: Section B.4.20,  Next: Section B.4.21,  Prev: Section B.4.19,  Up: Section B.4

B.4.20. `CLC', `CLD', `CLI', `CLTS': Clear Flags
------------------------------------------------

     CLC                           ; F8                   [8086]
     CLD                           ; FC                   [8086]
     CLI                           ; FA                   [8086]
     CLTS                          ; 0F 06                [286,PRIV]

   These instructions clear various flags. `CLC' clears the carry flag;
`CLD' clears the direction flag; `CLI' clears the interrupt flag (thus
disabling interrupts); and `CLTS' clears the task-switched (`TS') flag
in `CR0'.

   To set the carry, direction, or interrupt flags, use the `STC',
`STD' and `STI' instructions (*Note Section B.4.301::). To invert the
carry flag, use `CMC' (*Note Section B.4.22::).


File: nasm.info,  Node: Section B.4.21,  Next: Section B.4.22,  Prev: Section B.4.20,  Up: Section B.4

B.4.21. `CLFLUSH': Flush Cache Line
-----------------------------------

     CLFLUSH mem                   ; 0F AE /7        [WILLAMETTE,SSE2]

   `CLFLUSH' invalidates the cache line that contains the linear address
specified by the source operand from all levels of the processor cache
hierarchy (data and instruction). If, at any level of the cache
hierarchy, the line is inconsistent with memory (dirty) it is written
to memory before invalidation. The source operand points to a
byte-sized memory location.

   Although `CLFLUSH' is flagged `SSE2' and above, it may not be
present on all processors which have `SSE2' support, and it may be
supported on other processors; the `CPUID' instruction (*Note Section
B.4.34::) will return a bit which indicates support for the `CLFLUSH'
instruction.


File: nasm.info,  Node: Section B.4.22,  Next: Section B.4.23,  Prev: Section B.4.21,  Up: Section B.4

B.4.22. `CMC': Complement Carry Flag
------------------------------------

     CMC                           ; F5                   [8086]

   `CMC' changes the value of the carry flag: if it was 0, it sets it to
1, and vice versa.


File: nasm.info,  Node: Section B.4.23,  Next: Section B.4.24,  Prev: Section B.4.22,  Up: Section B.4

B.4.23. `CMOVcc': Conditional Move
----------------------------------

     CMOVcc reg16,r/m16            ; o16 0F 40+cc /r      [P6]
     CMOVcc reg32,r/m32            ; o32 0F 40+cc /r      [P6]

   `CMOV' moves its source (second) operand into its destination (first)
operand if the given condition code is satisfied; otherwise it does
nothing.

   For a list of condition codes, see *Note Section B.2.2::.

   Although the `CMOV' instructions are flagged `P6' and above, they
may not be supported by all Pentium Pro processors; the `CPUID'
instruction (*Note Section B.4.34::) will return a bit which indicates
whether conditional moves are supported.


File: nasm.info,  Node: Section B.4.24,  Next: Section B.4.25,  Prev: Section B.4.23,  Up: Section B.4

B.4.24. `CMP': Compare Integers
-------------------------------

     CMP r/m8,reg8                 ; 38 /r                [8086]
     CMP r/m16,reg16               ; o16 39 /r            [8086]
     CMP r/m32,reg32               ; o32 39 /r            [386]

     CMP reg8,r/m8                 ; 3A /r                [8086]
     CMP reg16,r/m16               ; o16 3B /r            [8086]
     CMP reg32,r/m32               ; o32 3B /r            [386]

     CMP r/m8,imm8                 ; 80 /0 ib             [8086]
     CMP r/m16,imm16               ; o16 81 /0 iw         [8086]
     CMP r/m32,imm32               ; o32 81 /0 id         [386]

     CMP r/m16,imm8                ; o16 83 /0 ib         [8086]
     CMP r/m32,imm8                ; o32 83 /0 ib         [386]

     CMP AL,imm8                   ; 3C ib                [8086]
     CMP AX,imm16                  ; o16 3D iw            [8086]
     CMP EAX,imm32                 ; o32 3D id            [386]

   `CMP' performs a `mental' subtraction of its second operand from its
first operand, and affects the flags as if the subtraction had taken
place, but does not store the result of the subtraction anywhere.

   In the forms with an 8-bit immediate second operand and a longer
first operand, the second operand is considered to be signed, and is
sign- extended to the length of the first operand. In these cases, the
`BYTE' qualifier is necessary to force NASM to generate this form of
the instruction.

   The destination operand can be a register or a memory location. The
source can be a register, memory location or an immediate value of the
same size as the destination.


File: nasm.info,  Node: Section B.4.25,  Next: Section B.4.26,  Prev: Section B.4.24,  Up: Section B.4

B.4.25. `CMPccPD': Packed Double-Precision FP Compare
-----------------------------------------------------

     CMPPD xmm1,xmm2/mem128,imm8   ; 66 0F C2 /r ib  [WILLAMETTE,SSE2]

     CMPEQPD xmm1,xmm2/mem128      ; 66 0F C2 /r 00  [WILLAMETTE,SSE2]
     CMPLTPD xmm1,xmm2/mem128      ; 66 0F C2 /r 01  [WILLAMETTE,SSE2]
     CMPLEPD xmm1,xmm2/mem128      ; 66 0F C2 /r 02  [WILLAMETTE,SSE2]
     CMPUNORDPD xmm1,xmm2/mem128   ; 66 0F C2 /r 03  [WILLAMETTE,SSE2]
     CMPNEQPD xmm1,xmm2/mem128     ; 66 0F C2 /r 04  [WILLAMETTE,SSE2]
     CMPNLTPD xmm1,xmm2/mem128     ; 66 0F C2 /r 05  [WILLAMETTE,SSE2]
     CMPNLEPD xmm1,xmm2/mem128     ; 66 0F C2 /r 06  [WILLAMETTE,SSE2]
     CMPORDPD xmm1,xmm2/mem128     ; 66 0F C2 /r 07  [WILLAMETTE,SSE2]

   The `CMPccPD' instructions compare the two packed double-precision FP
values in the source and destination operands, and returns the result of
the comparison in the destination register. The result of each
comparison is a quadword mask of all 1s (comparison true) or all 0s
(comparison false).

   The destination is an `XMM' register. The source can be either an
`XMM' register or a 128-bit memory location.

   The third operand is an 8-bit immediate value, of which the low 3
bits define the type of comparison. For ease of programming, the 8
two-operand pseudo-instructions are provided, with the third operand
already filled in.  The  `Condition Predicates' are:

     EQ     0   Equal
     LT     1   Less-than
     LE     2   Less-than-or-equal
     UNORD  3   Unordered
     NE     4   Not-equal
     NLT    5   Not-less-than
     NLE    6   Not-less-than-or-equal
     ORD    7   Ordered

   For more details of the comparison predicates, and details of how to
emulate the "greater-than" equivalents, see *Note Section B.2.3::


File: nasm.info,  Node: Section B.4.26,  Next: Section B.4.27,  Prev: Section B.4.25,  Up: Section B.4

B.4.26. `CMPccPS': Packed Single-Precision FP Compare
-----------------------------------------------------

     CMPPS xmm1,xmm2/mem128,imm8   ; 0F C2 /r ib     [KATMAI,SSE]

     CMPEQPS xmm1,xmm2/mem128      ; 0F C2 /r 00     [KATMAI,SSE]
     CMPLTPS xmm1,xmm2/mem128      ; 0F C2 /r 01     [KATMAI,SSE]
     CMPLEPS xmm1,xmm2/mem128      ; 0F C2 /r 02     [KATMAI,SSE]
     CMPUNORDPS xmm1,xmm2/mem128   ; 0F C2 /r 03     [KATMAI,SSE]
     CMPNEQPS xmm1,xmm2/mem128     ; 0F C2 /r 04     [KATMAI,SSE]
     CMPNLTPS xmm1,xmm2/mem128     ; 0F C2 /r 05     [KATMAI,SSE]
     CMPNLEPS xmm1,xmm2/mem128     ; 0F C2 /r 06     [KATMAI,SSE]
     CMPORDPS xmm1,xmm2/mem128     ; 0F C2 /r 07     [KATMAI,SSE]

   The `CMPccPS' instructions compare the two packed single-precision FP
values in the source and destination operands, and returns the result of
the comparison in the destination register. The result of each
comparison is a doubleword mask of all 1s (comparison true) or all 0s
(comparison false).

   The destination is an `XMM' register. The source can be either an
`XMM' register or a 128-bit memory location.

   The third operand is an 8-bit immediate value, of which the low 3
bits define the type of comparison. For ease of programming, the 8
two-operand pseudo-instructions are provided, with the third operand
already filled in.  The  `Condition Predicates' are:

     EQ     0   Equal
     LT     1   Less-than
     LE     2   Less-than-or-equal
     UNORD  3   Unordered
     NE     4   Not-equal
     NLT    5   Not-less-than
     NLE    6   Not-less-than-or-equal
     ORD    7   Ordered

   For more details of the comparison predicates, and details of how to
emulate the "greater-than" equivalents, see *Note Section B.2.3::


File: nasm.info,  Node: Section B.4.27,  Next: Section B.4.28,  Prev: Section B.4.26,  Up: Section B.4

B.4.27. `CMPSB', `CMPSW', `CMPSD': Compare Strings
--------------------------------------------------

     CMPSB                         ; A6                   [8086]
     CMPSW                         ; o16 A7               [8086]
     CMPSD                         ; o32 A7               [386]

   `CMPSB' compares the byte at `[DS:SI]' or `[DS:ESI]' with the byte
at `[ES:DI]' or `[ES:EDI]', and sets the flags accordingly. It then
increments or decrements (depending on the direction flag: increments
if the flag is clear, decrements if it is set) `SI' and `DI' (or `ESI'
and `EDI').

   The registers used are `SI' and `DI' if the address size is 16 bits,
and `ESI' and `EDI' if it is 32 bits. If you need to use an address
size not equal to the current `BITS' setting, you can use an explicit
`a16' or `a32' prefix.

   The segment register used to load from `[SI]' or `[ESI]' can be
overridden by using a segment register name as a prefix (for example,
`ES CMPSB'). The use of `ES' for the load from `[DI]' or `[EDI]' cannot
be overridden.

   `CMPSW' and `CMPSD' work in the same way, but they compare a word or
a doubleword instead of a byte, and increment or decrement the
addressing registers by 2 or 4 instead of 1.

   The `REPE' and `REPNE' prefixes (equivalently, `REPZ' and `REPNZ')
may be used to repeat the instruction up to `CX' (or `ECX' - again, the
address size chooses which) times until the first unequal or equal byte
is found.


File: nasm.info,  Node: Section B.4.28,  Next: Section B.4.29,  Prev: Section B.4.27,  Up: Section B.4

B.4.28. `CMPccSD': Scalar Double-Precision FP Compare
-----------------------------------------------------

     CMPSD xmm1,xmm2/mem64,imm8    ; F2 0F C2 /r ib  [WILLAMETTE,SSE2]

     CMPEQSD xmm1,xmm2/mem64       ; F2 0F C2 /r 00  [WILLAMETTE,SSE2]
     CMPLTSD xmm1,xmm2/mem64       ; F2 0F C2 /r 01  [WILLAMETTE,SSE2]
     CMPLESD xmm1,xmm2/mem64       ; F2 0F C2 /r 02  [WILLAMETTE,SSE2]
     CMPUNORDSD xmm1,xmm2/mem64    ; F2 0F C2 /r 03  [WILLAMETTE,SSE2]
     CMPNEQSD xmm1,xmm2/mem64      ; F2 0F C2 /r 04  [WILLAMETTE,SSE2]
     CMPNLTSD xmm1,xmm2/mem64      ; F2 0F C2 /r 05  [WILLAMETTE,SSE2]
     CMPNLESD xmm1,xmm2/mem64      ; F2 0F C2 /r 06  [WILLAMETTE,SSE2]
     CMPORDSD xmm1,xmm2/mem64      ; F2 0F C2 /r 07  [WILLAMETTE,SSE2]

   The `CMPccSD' instructions compare the low-order double-precision FP
values in the source and destination operands, and returns the result of
the comparison in the destination register. The result of each
comparison is a quadword mask of all 1s (comparison true) or all 0s
(comparison false).

   The destination is an `XMM' register. The source can be either an
`XMM' register or a 128-bit memory location.

   The third operand is an 8-bit immediate value, of which the low 3
bits define the type of comparison. For ease of programming, the 8
two-operand pseudo-instructions are provided, with the third operand
already filled in.  The  `Condition Predicates' are:

     EQ     0   Equal
     LT     1   Less-than
     LE     2   Less-than-or-equal
     UNORD  3   Unordered
     NE     4   Not-equal
     NLT    5   Not-less-than
     NLE    6   Not-less-than-or-equal
     ORD    7   Ordered

   For more details of the comparison predicates, and details of how to
emulate the "greater-than" equivalents, see *Note Section B.2.3::


File: nasm.info,  Node: Section B.4.29,  Next: Section B.4.30,  Prev: Section B.4.28,  Up: Section B.4

B.4.29. `CMPccSS': Scalar Single-Precision FP Compare
-----------------------------------------------------

     CMPSS xmm1,xmm2/mem32,imm8    ; F3 0F C2 /r ib  [KATMAI,SSE]

     CMPEQSS xmm1,xmm2/mem32       ; F3 0F C2 /r 00  [KATMAI,SSE]
     CMPLTSS xmm1,xmm2/mem32       ; F3 0F C2 /r 01  [KATMAI,SSE]
     CMPLESS xmm1,xmm2/mem32       ; F3 0F C2 /r 02  [KATMAI,SSE]
     CMPUNORDSS xmm1,xmm2/mem32    ; F3 0F C2 /r 03  [KATMAI,SSE]
     CMPNEQSS xmm1,xmm2/mem32      ; F3 0F C2 /r 04  [KATMAI,SSE]
     CMPNLTSS xmm1,xmm2/mem32      ; F3 0F C2 /r 05  [KATMAI,SSE]
     CMPNLESS xmm1,xmm2/mem32      ; F3 0F C2 /r 06  [KATMAI,SSE]
     CMPORDSS xmm1,xmm2/mem32      ; F3 0F C2 /r 07  [KATMAI,SSE]

   The `CMPccSS' instructions compare the low-order single-precision FP
values in the source and destination operands, and returns the result of
the comparison in the destination register. The result of each
comparison is a doubleword mask of all 1s (comparison true) or all 0s
(comparison false).

   The destination is an `XMM' register. The source can be either an
`XMM' register or a 128-bit memory location.

   The third operand is an 8-bit immediate value, of which the low 3
bits define the type of comparison. For ease of programming, the 8
two-operand pseudo-instructions are provided, with the third operand
already filled in.  The  `Condition Predicates' are:

     EQ     0   Equal
     LT     1   Less-than
     LE     2   Less-than-or-equal
     UNORD  3   Unordered
     NE     4   Not-equal
     NLT    5   Not-less-than
     NLE    6   Not-less-than-or-equal
     ORD    7   Ordered

   For more details of the comparison predicates, and details of how to
emulate the "greater-than" equivalents, see *Note Section B.2.3::


File: nasm.info,  Node: Section B.4.30,  Next: Section B.4.31,  Prev: Section B.4.29,  Up: Section B.4

B.4.30. `CMPXCHG', `CMPXCHG486': Compare and Exchange
-----------------------------------------------------

     CMPXCHG r/m8,reg8             ; 0F B0 /r             [PENT]
     CMPXCHG r/m16,reg16           ; o16 0F B1 /r         [PENT]
     CMPXCHG r/m32,reg32           ; o32 0F B1 /r         [PENT]

     CMPXCHG486 r/m8,reg8          ; 0F A6 /r             [486,UNDOC]
     CMPXCHG486 r/m16,reg16        ; o16 0F A7 /r         [486,UNDOC]
     CMPXCHG486 r/m32,reg32        ; o32 0F A7 /r         [486,UNDOC]

   These two instructions perform exactly the same operation; however,
apparently some (not all) 486 processors support it under a non-standard
opcode, so NASM provides the undocumented `CMPXCHG486' form to generate
the non-standard opcode.

   `CMPXCHG' compares its destination (first) operand to the value in
`AL', `AX' or `EAX' (depending on the operand size of the instruction).
If they are equal, it copies its source (second) operand into the
destination and sets the zero flag. Otherwise, it clears the zero flag
and copies the destination register to AL, AX or EAX.

   The destination can be either a register or a memory location. The
source is a register.

   `CMPXCHG' is intended to be used for atomic operations in
multitasking or multiprocessor environments. To safely update a value
in shared memory, for example, you might load the value into `EAX',
load the updated value into `EBX', and then execute the instruction
`LOCK CMPXCHG [value],EBX'. If `value' has not changed since being
loaded, it is updated with your desired new value, and the zero flag is
set to let you know it has worked. (The `LOCK' prefix prevents another
processor doing anything in the middle of this operation: it guarantees
atomicity.) However, if another processor has modified the value in
between your load and your attempted store, the store does not happen,
and you are notified of the failure by a cleared zero flag, so you can
go round and try again.


File: nasm.info,  Node: Section B.4.31,  Next: Section B.4.32,  Prev: Section B.4.30,  Up: Section B.4

B.4.31. `CMPXCHG8B': Compare and Exchange Eight Bytes
-----------------------------------------------------

     CMPXCHG8B mem                 ; 0F C7 /1             [PENT]

   This is a larger and more unwieldy version of `CMPXCHG': it compares
the 64-bit (eight-byte) value stored at `[mem]' with the value in
`EDX:EAX'. If they are equal, it sets the zero flag and stores
`ECX:EBX' into the memory area. If they are unequal, it clears the zero
flag and stores the memory contents into `EDX:EAX'.

   `CMPXCHG8B' can be used with the `LOCK' prefix, to allow atomic
execution. This is useful in multi-processor and multi-tasking
environments.


File: nasm.info,  Node: Section B.4.32,  Next: Section B.4.33,  Prev: Section B.4.31,  Up: Section B.4

B.4.32. `COMISD': Scalar Ordered Double-Precision FP Compare and Set EFLAGS
---------------------------------------------------------------------------

     COMISD xmm1,xmm2/mem64        ; 66 0F 2F /r     [WILLAMETTE,SSE2]

   `COMISD' compares the low-order double-precision FP value in the two
source operands. ZF, PF and CF are set according to the result. OF, AF
and AF are cleared. The unordered result is returned if either source
is a NaN (QNaN or SNaN).

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a memory location.

   The flags are set according to the following rules:

        Result          Flags        Values

        UNORDERED:      ZF,PF,CF <-- 111;
        GREATER_THAN:   ZF,PF,CF <-- 000;
        LESS_THAN:      ZF,PF,CF <-- 001;
        EQUAL:          ZF,PF,CF <-- 100;


File: nasm.info,  Node: Section B.4.33,  Next: Section B.4.34,  Prev: Section B.4.32,  Up: Section B.4

B.4.33. `COMISS': Scalar Ordered Single-Precision FP Compare and Set EFLAGS
---------------------------------------------------------------------------

     COMISS xmm1,xmm2/mem32        ; 66 0F 2F /r     [KATMAI,SSE]

   `COMISS' compares the low-order single-precision FP value in the two
source operands. ZF, PF and CF are set according to the result. OF, AF
and AF are cleared. The unordered result is returned if either source
is a NaN (QNaN or SNaN).

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a memory location.

   The flags are set according to the following rules:

        Result          Flags        Values

        UNORDERED:      ZF,PF,CF <-- 111;
        GREATER_THAN:   ZF,PF,CF <-- 000;
        LESS_THAN:      ZF,PF,CF <-- 001;
        EQUAL:          ZF,PF,CF <-- 100;


File: nasm.info,  Node: Section B.4.34,  Next: Section B.4.35,  Prev: Section B.4.33,  Up: Section B.4

B.4.34. `CPUID': Get CPU Identification Code
--------------------------------------------

     CPUID                         ; 0F A2                [PENT]

   `CPUID' returns various information about the processor it is being
executed on. It fills the four registers `EAX', `EBX', `ECX' and `EDX'
with information, which varies depending on the input contents of `EAX'.

   `CPUID' also acts as a barrier to serialise instruction execution:
executing the `CPUID' instruction guarantees that all the effects
(memory modification, flag modification, register modification) of
previous instructions have been completed before the next instruction
gets fetched.

   The information returned is as follows:

   * If `EAX' is zero on input, `EAX' on output holds the maximum
     acceptable input value of `EAX', and `EBX:EDX:ECX' contain the
     string `"GenuineIntel"' (or not, if you have a clone processor).
     That is to say, `EBX' contains `"Genu"' (in NASM's own sense of
     character constants, described in *Note Section 3.4.2::), `EDX'
     contains `"ineI"' and `ECX' contains `"ntel"'.

   * If `EAX' is one on input, `EAX' on output contains version
     information about the processor, and `EDX' contains a set of
     feature flags, showing the presence and absence of various
     features. For example, bit 8 is set if the `CMPXCHG8B' instruction
     (*Note Section B.4.31::) is supported, bit 15 is set if the
     conditional move instructions (*Note Section B.4.23:: and *Note
     Section B.4.72::) are supported, and bit 23 is set if `MMX'
     instructions are supported.

   * If `EAX' is two on input, `EAX', `EBX', `ECX' and `EDX' all
     contain information about caches and TLBs (Translation Lookahead
     Buffers).

   For more information on the data returned from `CPUID', see the
documentation from Intel and other processor manufacturers.


File: nasm.info,  Node: Section B.4.35,  Next: Section B.4.36,  Prev: Section B.4.34,  Up: Section B.4

B.4.35. `CVTDQ2PD': Packed Signed INT32 to Packed Double-Precision FP Conversion
--------------------------------------------------------------------------------

     CVTDQ2PD xmm1,xmm2/mem64      ; F3 0F E6 /r     [WILLAMETTE,SSE2]

   `CVTDQ2PD' converts two packed signed doublewords from the source
operand to two packed double-precision FP values in the destination
operand.

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a 64-bit memory location. If the source is a
register, the packed integers are in the low quadword.


File: nasm.info,  Node: Section B.4.36,  Next: Section B.4.37,  Prev: Section B.4.35,  Up: Section B.4

B.4.36. `CVTDQ2PS': Packed Signed INT32 to Packed Single-Precision FP Conversion
--------------------------------------------------------------------------------

     CVTDQ2PS xmm1,xmm2/mem128     ; 0F 5B /r        [WILLAMETTE,SSE2]

   `CVTDQ2PS' converts four packed signed doublewords from the source
operand to four packed single-precision FP values in the destination
operand.

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a 128-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.37,  Next: Section B.4.38,  Prev: Section B.4.36,  Up: Section B.4

B.4.37. `CVTPD2DQ': Packed Double-Precision FP to Packed Signed INT32 Conversion
--------------------------------------------------------------------------------

     CVTPD2DQ xmm1,xmm2/mem128     ; F2 0F E6 /r     [WILLAMETTE,SSE2]

   `CVTPD2DQ' converts two packed double-precision FP values from the
source operand to two packed signed doublewords in the low quadword of
the destination operand. The high quadword of the destination is set to
all 0s.

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a 128-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.38,  Next: Section B.4.39,  Prev: Section B.4.37,  Up: Section B.4

B.4.38. `CVTPD2PI': Packed Double-Precision FP to Packed Signed INT32 Conversion
--------------------------------------------------------------------------------

     CVTPD2PI mm,xmm/mem128        ; 66 0F 2D /r     [WILLAMETTE,SSE2]

   `CVTPD2PI' converts two packed double-precision FP values from the
source operand to two packed signed doublewords in the destination
operand.

   The destination operand is an `MMX' register. The source can be
either an `XMM' register or a 128-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.39,  Next: Section B.4.40,  Prev: Section B.4.38,  Up: Section B.4

B.4.39. `CVTPD2PS': Packed Double-Precision FP to Packed Single-Precision FP Conversion
---------------------------------------------------------------------------------------

     CVTPD2PS xmm1,xmm2/mem128     ; 66 0F 5A /r     [WILLAMETTE,SSE2]

   `CVTPD2PS' converts two packed double-precision FP values from the
source operand to two packed single-precision FP values in the low
quadword of the destination operand. The high quadword of the
destination is set to all 0s.

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a 128-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.40,  Next: Section B.4.41,  Prev: Section B.4.39,  Up: Section B.4

B.4.40. `CVTPI2PD': Packed Signed INT32 to Packed Double-Precision FP Conversion
--------------------------------------------------------------------------------

     CVTPI2PD xmm,mm/mem64         ; 66 0F 2A /r     [WILLAMETTE,SSE2]

   `CVTPI2PD' converts two packed signed doublewords from the source
operand to two packed double-precision FP values in the destination
operand.

   The destination operand is an `XMM' register. The source can be
either an `MMX' register or a 64-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.41,  Next: Section B.4.42,  Prev: Section B.4.40,  Up: Section B.4

B.4.41. `CVTPI2PS': Packed Signed INT32 to Packed Single-FP Conversion
----------------------------------------------------------------------

     CVTPI2PS xmm,mm/mem64         ; 0F 2A /r        [KATMAI,SSE]

   `CVTPI2PS' converts two packed signed doublewords from the source
operand to two packed single-precision FP values in the low quadword of
the destination operand. The high quadword of the destination remains
unchanged.

   The destination operand is an `XMM' register. The source can be
either an `MMX' register or a 64-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.42,  Next: Section B.4.43,  Prev: Section B.4.41,  Up: Section B.4

B.4.42. `CVTPS2DQ': Packed Single-Precision FP to Packed Signed INT32 Conversion
--------------------------------------------------------------------------------

     CVTPS2DQ xmm1,xmm2/mem128     ; 66 0F 5B /r     [WILLAMETTE,SSE2]

   `CVTPS2DQ' converts four packed single-precision FP values from the
source operand to four packed signed doublewords in the destination
operand.

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a 128-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.43,  Next: Section B.4.44,  Prev: Section B.4.42,  Up: Section B.4

B.4.43. `CVTPS2PD': Packed Single-Precision FP to Packed Double-Precision FP Conversion
---------------------------------------------------------------------------------------

     CVTPS2PD xmm1,xmm2/mem64      ; 0F 5A /r        [WILLAMETTE,SSE2]

   `CVTPS2PD' converts two packed single-precision FP values from the
source operand to two packed double-precision FP values in the
destination operand.

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a 64-bit memory location. If the source is a
register, the input values are in the low quadword.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.44,  Next: Section B.4.45,  Prev: Section B.4.43,  Up: Section B.4

B.4.44. `CVTPS2PI': Packed Single-Precision FP to Packed Signed INT32 Conversion
--------------------------------------------------------------------------------

     CVTPS2PI mm,xmm/mem64         ; 0F 2D /r        [KATMAI,SSE]

   `CVTPS2PI' converts two packed single-precision FP values from the
source operand to two packed signed doublewords in the destination
operand.

   The destination operand is an `MMX' register. The source can be
either an `XMM' register or a 64-bit memory location. If the source is a
register, the input values are in the low quadword.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.45,  Next: Section B.4.46,  Prev: Section B.4.44,  Up: Section B.4

B.4.45. `CVTSD2SI': Scalar Double-Precision FP to Signed INT32 Conversion
-------------------------------------------------------------------------

     CVTSD2SI reg32,xmm/mem64      ; F2 0F 2D /r     [WILLAMETTE,SSE2]

   `CVTSD2SI' converts a double-precision FP value from the source
operand to a signed doubleword in the destination operand.

   The destination operand is a general purpose register. The source
can be either an `XMM' register or a 64-bit memory location. If the
source is a register, the input value is in the low quadword.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.46,  Next: Section B.4.47,  Prev: Section B.4.45,  Up: Section B.4

B.4.46. `CVTSD2SS': Scalar Double-Precision FP to Scalar Single-Precision FP Conversion
---------------------------------------------------------------------------------------

     CVTSD2SS xmm1,xmm2/mem64      ; F2 0F 5A /r     [KATMAI,SSE]

   `CVTSD2SS' converts a double-precision FP value from the source
operand to a single-precision FP value in the low doubleword of the
destination operand. The upper 3 doublewords are left unchanged.

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a 64-bit memory location. If the source is a
register, the input value is in the low quadword.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.47,  Next: Section B.4.48,  Prev: Section B.4.46,  Up: Section B.4

B.4.47. `CVTSI2SD': Signed INT32 to Scalar Double-Precision FP Conversion
-------------------------------------------------------------------------

     CVTSI2SD xmm,r/m32            ; F2 0F 2A /r     [WILLAMETTE,SSE2]

   `CVTSI2SD' converts a signed doubleword from the source operand to a
double-precision FP value in the low quadword of the destination
operand.  The high quadword is left unchanged.

   The destination operand is an `XMM' register. The source can be
either a general purpose register or a 32-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.48,  Next: Section B.4.49,  Prev: Section B.4.47,  Up: Section B.4

B.4.48. `CVTSI2SS': Signed INT32 to Scalar Single-Precision FP Conversion
-------------------------------------------------------------------------

     CVTSI2SS xmm,r/m32            ; F3 0F 2A /r     [KATMAI,SSE]

   `CVTSI2SS' converts a signed doubleword from the source operand to a
single-precision FP value in the low doubleword of the destination
operand.  The upper 3 doublewords are left unchanged.

   The destination operand is an `XMM' register. The source can be
either a general purpose register or a 32-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.49,  Next: Section B.4.50,  Prev: Section B.4.48,  Up: Section B.4

B.4.49. `CVTSS2SD': Scalar Single-Precision FP to Scalar Double-Precision FP Conversion
---------------------------------------------------------------------------------------

     CVTSS2SD xmm1,xmm2/mem32      ; F3 0F 5A /r     [WILLAMETTE,SSE2]

   `CVTSS2SD' converts a single-precision FP value from the source
operand to a double-precision FP value in the low quadword of the
destination operand. The upper quadword is left unchanged.

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a 32-bit memory location. If the source is a
register, the input value is contained in the low doubleword.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.50,  Next: Section B.4.51,  Prev: Section B.4.49,  Up: Section B.4

B.4.50. `CVTSS2SI': Scalar Single-Precision FP to Signed INT32 Conversion
-------------------------------------------------------------------------

     CVTSS2SI reg32,xmm/mem32      ; F3 0F 2D /r     [KATMAI,SSE]

   `CVTSS2SI' converts a single-precision FP value from the source
operand to a signed doubleword in the destination operand.

   The destination operand is a general purpose register. The source
can be either an `XMM' register or a 32-bit memory location. If the
source is a register, the input value is in the low doubleword.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.51,  Next: Section B.4.52,  Prev: Section B.4.50,  Up: Section B.4

B.4.51. `CVTTPD2DQ': Packed Double-Precision FP to Packed Signed INT32 Conversion with Truncation
-------------------------------------------------------------------------------------------------

     CVTTPD2DQ xmm1,xmm2/mem128    ; 66 0F E6 /r     [WILLAMETTE,SSE2]

   `CVTTPD2DQ' converts two packed double-precision FP values in the
source operand to two packed single-precision FP values in the
destination operand. If the result is inexact, it is truncated (rounded
toward zero).  The high quadword is set to all 0s.

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a 128-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.52,  Next: Section B.4.53,  Prev: Section B.4.51,  Up: Section B.4

B.4.52. `CVTTPD2PI': Packed Double-Precision FP to Packed Signed INT32 Conversion with Truncation
-------------------------------------------------------------------------------------------------

     CVTTPD2PI mm,xmm/mem128        ; 66 0F 2C /r     [WILLAMETTE,SSE2]

   `CVTTPD2PI' converts two packed double-precision FP values in the
source operand to two packed single-precision FP values in the
destination operand. If the result is inexact, it is truncated (rounded
toward zero).

   The destination operand is an `MMX' register. The source can be
either an `XMM' register or a 128-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.53,  Next: Section B.4.54,  Prev: Section B.4.52,  Up: Section B.4

B.4.53. `CVTTPS2DQ': Packed Single-Precision FP to Packed Signed INT32 Conversion with Truncation
-------------------------------------------------------------------------------------------------

     CVTTPS2DQ xmm1,xmm2/mem128    ; F3 0F 5B /r     [WILLAMETTE,SSE2]

   `CVTTPS2DQ' converts four packed single-precision FP values in the
source operand to four packed signed doublewords in the destination
operand. If the result is inexact, it is truncated (rounded toward
zero).

   The destination operand is an `XMM' register. The source can be
either an `XMM' register or a 128-bit memory location.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.54,  Next: Section B.4.55,  Prev: Section B.4.53,  Up: Section B.4

B.4.54. `CVTTPS2PI': Packed Single-Precision FP to Packed Signed INT32 Conversion with Truncation
-------------------------------------------------------------------------------------------------

     CVTTPS2PI mm,xmm/mem64         ; 0F 2C /r       [KATMAI,SSE]

   `CVTTPS2PI' converts two packed single-precision FP values in the
source operand to two packed signed doublewords in the destination
operand.  If the result is inexact, it is truncated (rounded toward
zero). If the source is a register, the input values are in the low
quadword.

   The destination operand is an `MMX' register. The source can be
either an `XMM' register or a 64-bit memory location. If the source is a
register, the input value is in the low quadword.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.55,  Next: Section B.4.56,  Prev: Section B.4.54,  Up: Section B.4

B.4.55. `CVTTSD2SI': Scalar Double-Precision FP to Signed INT32 Conversion with Truncation
------------------------------------------------------------------------------------------

     CVTTSD2SI reg32,xmm/mem64      ; F2 0F 2C /r    [WILLAMETTE,SSE2]

   `CVTTSD2SI' converts a double-precision FP value in the source
operand to a signed doubleword in the destination operand. If the
result is inexact, it is truncated (rounded toward zero).

   The destination operand is a general purpose register. The source
can be either an `XMM' register or a 64-bit memory location. If the
source is a register, the input value is in the low quadword.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.56,  Next: Section B.4.57,  Prev: Section B.4.55,  Up: Section B.4

B.4.56. `CVTTSS2SI': Scalar Single-Precision FP to Signed INT32 Conversion with Truncation
------------------------------------------------------------------------------------------

     CVTTSD2SI reg32,xmm/mem32      ; F3 0F 2C /r    [KATMAI,SSE]

   `CVTTSS2SI' converts a single-precision FP value in the source
operand to a signed doubleword in the destination operand. If the
result is inexact, it is truncated (rounded toward zero).

   The destination operand is a general purpose register. The source
can be either an `XMM' register or a 32-bit memory location. If the
source is a register, the input value is in the low doubleword.

   For more details of this instruction, see the Intel Processor
manuals.


File: nasm.info,  Node: Section B.4.57,  Next: Section B.4.58,  Prev: Section B.4.56,  Up: Section B.4

B.4.57. `DAA', `DAS': Decimal Adjustments
-----------------------------------------

     DAA                           ; 27                   [8086]
     DAS                           ; 2F                   [8086]

   These instructions are used in conjunction with the add and subtract
instructions to perform binary-coded decimal arithmetic in _packed_
(one BCD digit per nibble) form. For the unpacked equivalents, see
*Note Section B.4.1::.

   `DAA' should be used after a one-byte `ADD' instruction whose
destination was the `AL' register: by means of examining the value in
the `AL' and also the auxiliary carry flag `AF', it determines whether
either digit of the addition has overflowed, and adjusts it (and sets
the carry and auxiliary-carry flags) if so. You can add long BCD
strings together by doing `ADD'/`DAA' on the low two digits, then doing
`ADC'/`DAA' on each subsequent pair of digits.

   `DAS' works similarly to `DAA', but is for use after `SUB'
instructions rather than `ADD'.


File: nasm.info,  Node: Section B.4.58,  Next: Section B.4.59,  Prev: Section B.4.57,  Up: Section B.4

B.4.58. `DEC': Decrement Integer
--------------------------------

     DEC reg16                     ; o16 48+r             [8086]
     DEC reg32                     ; o32 48+r             [386]
     DEC r/m8                      ; FE /1                [8086]
     DEC r/m16                     ; o16 FF /1            [8086]
     DEC r/m32                     ; o32 FF /1            [386]

   `DEC' subtracts 1 from its operand. It does _not_ affect the carry
flag: to affect the carry flag, use `SUB something,1' (see *Note
Section B.4.305::). `DEC' affects all the other flags according to the
result.

   This instruction can be used with a `LOCK' prefix to allow atomic
execution.

   See also `INC' (*Note Section B.4.120::).


File: nasm.info,  Node: Section B.4.59,  Next: Section B.4.60,  Prev: Section B.4.58,  Up: Section B.4

B.4.59. `DIV': Unsigned Integer Divide
--------------------------------------

     DIV r/m8                      ; F6 /6                [8086]
     DIV r/m16                     ; o16 F7 /6            [8086]
     DIV r/m32                     ; o32 F7 /6            [386]

   `DIV' performs unsigned integer division. The explicit operand
provided is the divisor; the dividend and destination operands are
implicit, in the following way:

   * For `DIV r/m8', `AX' is divided by the given operand; the quotient
     is stored in `AL' and the remainder in `AH'.

   * For `DIV r/m16', `DX:AX' is divided by the given operand; the
     quotient is stored in `AX' and the remainder in `DX'.

   * For `DIV r/m32', `EDX:EAX' is divided by the given operand; the
     quotient is stored in `EAX' and the remainder in `EDX'.

   Signed integer division is performed by the `IDIV' instruction: see
*Note Section B.4.117::.


File: nasm.info,  Node: Section B.4.60,  Next: Section B.4.61,  Prev: Section B.4.59,  Up: Section B.4

B.4.60. `DIVPD': Packed Double-Precision FP Divide
--------------------------------------------------

     DIVPD xmm1,xmm2/mem128        ; 66 0F 5E /r     [WILLAMETTE,SSE2]

   `DIVPD' divides the two packed double-precision FP values in the
destination operand by the two packed double-precision FP values in the
source operand, and stores the packed double-precision results in the
destination register.

   The destination is an `XMM' register. The source operand can be
either an `XMM' register or a 128-bit memory location.

        dst[0-63]   := dst[0-63]   / src[0-63],
        dst[64-127] := dst[64-127] / src[64-127].


File: nasm.info,  Node: Section B.4.61,  Next: Section B.4.62,  Prev: Section B.4.60,  Up: Section B.4

B.4.61. `DIVPS': Packed Single-Precision FP Divide
--------------------------------------------------

     DIVPS xmm1,xmm2/mem128        ; 0F 5E /r        [KATMAI,SSE]

   `DIVPS' divides the four packed single-precision FP values in the
destination operand by the four packed single-precision FP values in the
source operand, and stores the packed single-precision results in the
destination register.

   The destination is an `XMM' register. The source operand can be
either an `XMM' register or a 128-bit memory location.

        dst[0-31]   := dst[0-31]   / src[0-31],
        dst[32-63]  := dst[32-63]  / src[32-63],
        dst[64-95]  := dst[64-95]  / src[64-95],
        dst[96-127] := dst[96-127] / src[96-127].

