##

# Members

#### # global

##### Properties:

Name | Type | Description
--- | --- | ---
`global` | `object` | the global context.

#### # PDF_A3_HEIGHT

DIN A3 page height

#### # PDF_A3_WIDTH

DIN A3 page width

#### # PDF_A4_HEIGHT

DIN A4 page height

#### # PDF_A4_WIDTH

DIN A4 page width

#### # PDF_ALIGN_CENTER

align text center

#### # PDF_ALIGN_JUSTIFY

align text in the center, with padding to fill the available space

#### # PDF_ALIGN_JUSTIFY_ALL

Like PDF_ALIGN_JUSTIFY, except even short lines will be fully justified

#### # PDF_ALIGN_LEFT

align text left

#### # PDF_ALIGN_NO_WRITE

Fake alignment for only checking wrap height with no writes

#### # PDF_ALIGN_RIGHT

align text right

#### # PDF_BARCODE_39

Produce code-39 style barcodes

#### # PDF_BARCODE_128A

Produce code-128A style barcodes

#### # PDF_COURIER

PDf font.

#### # PDF_COURIER_BOLD

PDf font.

#### # PDF_COURIER_BOLD_OBLIQUE

PDf font.

#### # PDF_COURIER_OBLIQUE

PDf font.

#### # PDF_HELVETICA

PDf font.

#### # PDF_HELVETICA_BOLD

PDf font.

#### # PDF_HELVETICA_BOLD_OBLIQUE

PDf font.

#### # PDF_HELVETICA_OBLIQUE

PDf font.

#### # PDF_LETTER_HEIGHT

LETTER page height

#### # PDF_LETTER_WIDTH

LETTER page width

#### # PDF_SYMBOL

PDf font.

#### # PDF_TIMES

PDf font.

#### # PDF_TIMES_BOLD

PDf font.

#### # PDF_TIMES_BOLD_OBLIQUE

PDf font.

#### # PDF_TIMES_OBLIQUE

PDf font.

#### # PDF_TOPLEVEL_BOOKMARK

id for top-level bookmark.

#### # PDF_ZAPF_DINGBATS

PDf font.

# Methods

#### # Input(event)

This function is called whenever mouse / keyboard input happens.

##### Parameters:

Name | Type | Description
--- | --- | ---
`event` | `Event` | the current event.

#### # Loop()

This function is called after setup repeatedly until Stop is called. After calling Stop the program ends when Loop exits.

#### # MakeQR(bmw, bmh, text) → {Bitmap}

Create a QR code as Bitmap

##### Parameters:

Name | Type | Description
--- | --- | ---
`bmw` | `Number` | width of the wanted bitmap
`bmh` | `Number` | height of the wanted bitmap
`text` | `String` | the text to encode into the QR code.

Returns:

a bitmap containing a QR code.

Type: `Bitmap`

#### # Setup()

This function is called once at startup. It can initialize variables, setup hardware, etc.

# Type Definitions

Type: `object`

#### # ArcInfo

An object with coordinates of a drawn arc.

##### Properties:

Name | Type | Description
--- | --- | ---
`centerX` | `number` | center x coordinate of the arc.
`centerY` | `number` | center y coordinate of the arc.
`startX` | `number` | x coordinate of the arc start.
`startY` | `number` | y coordinate of the arc start.
`endX` | `number` | x coordinate of the arc end.
`endY` | `number` | y coordinate of the arc end.

Type: `object`

#### # CpuInfo

complex object containing the state information for all buttons and sticks. "-1" means "not available"

##### Example

    {
    	"brand_str": "",
    	"cpu_clock": 55,
    	"cpu_clock_measure": 62,
    	"cpu_codename": "i486 DX-25/33",
    	"ext_family": 4,
    	"ext_model": 0,
    	"family": 4,
    	"features": [
    		"fpu"
    	],
    	"l1_data_assoc": -1,
    	"l1_data_cache": -1,
    	"l1_data_cacheline": -1,
    	"l1_instruction_assoc": -1,
    	"l1_instruction_cache": -1,
    	"l1_instruction_cacheline": -1,
    	"l2_assoc": -1,
    	"l2_cache": -1,
    	"l2_cacheline": -1,
    	"l3_assoc": -1,
    	"l3_cache": -1,
    	"l3_cacheline": -1,
    	"l4_assoc": -1,
    	"l4_cache": -1,
    	"l4_cacheline": -1,
    	"model": 0,
    	"num_cores": 1,
    	"num_logical_cpus": 1,
    	"sse_size": -1,
    	"stepping": 2,
    	"total_logical_cpus": 1,
    	"vendor": 0,
    	"vendor_str": "GenuineIntel"
    }

Type: `object`

#### # Event

##### Properties:

Name | Type | Description
--- | --- | ---
`x` | `number` | mouse X coordinate.
`y` | `number` | mouse X coordinate.
`buttons` | `number` | mouse buttons, see MOUSE
`key` | `number` | key code, see KEY
`ticks` | `number` | event time.

Type: `object`

#### # HTTPResult

An array with the HTTP result: [code, message, header, data]

Type: `object`

#### # IpAdddress

An array with four numbers (e.g. [192.168.1.2]).

Type: `object`

#### # IpcAddress

Node addresses are arrays of 6 numbers between 0-255 (e.g. [1, 2, 3, 4, 5, 6]).

Type: `object`

#### # IpxPacket

received IPX data packet.

##### Properties:

Name | Type | Description
--- | --- | ---
`data` | `string` | the received data.
`source` | `IpxAddress` | address of the sending node.

Type: `object`

#### # Matrix

##### Properties:

Name | Type | Description
--- | --- | ---
`v` | `Array.<Array.<number>>` | the 3x3 matrix data.
`t` | `Array.<number>` | the translation data.

Type: `object`

#### # MemInfo

##### Properties:

Name | Type | Description
--- | --- | ---
`total` | `number` | total amount of memory in the system.
`remaining` | `number` | number of available bytes.

Type: `object`

#### # Node

The root node of the QuadTree which covers the entire area being segmented.

##### Properties:

Name | Type | Description
--- | --- | ---
`root` |  |

Type: `object`

#### # StatInfo

##### Properties:

Name | Type | Description
--- | --- | ---
`atime` | `string` | file access timestamp.
`ctime` | `string` | file creation time.
`mtime` | `string` | file modification time.
`blksize` | `number` | file size in blocks.
`size` | `number` | file size in bytes.
`nlink` | `number` | number of sub entries.
`drive` | `string` | drive letter for the entry.
`is_blockdev` | `boolean` | true if this is a block device.
`is_chardev` | `boolean` | true if this is a character device.
`is_directory` | `boolean` | true if this is a directory.
`is_regular` | `boolean` | true if this is a regular file.