
ODIPKT provides a packet driver interface over ODI drivers. May modern ethernet card manufacturer's don't provide DOS packet drivers anymore. But they will often provide ODI drivers for use with Novell networking software. ODIPKT can turn these ODI drivers into a packet driver that Ikon can use for it's networking applications.

You will need to find an ODI driver for your ethernet card on the manufacturer's website. Then edit the "net.cfg" configuration file that *should* come with the driver. A sample net.cfg file is listed below:

;*******************  NET.CFG *********************
Link Support
        buffers 6, 1600

Protocol IPX


; NOTE: Bind this to the ODI driver for your card.
; The line below uses YUKODI.COM for Marvell Yukon cards
; which is included in c:\ikon\drivers\net directory
        Bind YUKODI
Link Driver YUKODI

; NOTE: Be sure envelope type is ETHERNET_II
        envelope type ETHERNET_II

;***************************************************

Once you have saved your custom net.cfg file to c:\ikon\drivers\net\net.cfg then
you can add the following to c:\ikon\ikon.bat in place of "LOADHIGH ne2000 0x60".

cd\drivers\net <-----------Go to drivers directory where net.cfg is
LOADHIGH lsl
LOADHIGH yukodi   <------- Replace with the ODI driver for your card.
LOADHIGH odipkt 0 96  <--- This sets up the packet driver on interrupt 0x60 -> 96 decimal
cd\ikon

That's it. You should be able to use Ikon's internet applications.
