(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 102.87 103.94)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Fab_output_files/")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (net 3 "+5V")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D3-Pad1)")
  (net 9 "Net-(D3-Pad2)")
  (net 10 "Net-(D4-Pad1)")
  (net 11 "+9V")
  (net 12 "Net-(R1-Pad2)")
  (net 13 "TRIP")
  (net 14 "Net-(R3-Pad2)")
  (net 15 "Net-(R6-Pad2)")
  (net 16 "SENSE")
  (net 17 "Net-(C3-Pad2)")
  (net 18 "Net-(RV1-Pad2)")
  (net 19 "Net-(RV2-Pad2)")
  (net 20 "Net-(U1-Pad2)")
  (net 21 "Net-(U1-Pad3)")
  (net 22 "Net-(U1-Pad10)")
  (net 23 "LINE")
  (net 24 "LOAD")
  (footprint "" (layer "F.Cu")
    (at 121.92 78.74)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(RV1-Pad2)") (pinfunction "Pin_1") (pintype "passive") (zone_connect 2))
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 172.39 106.68 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R11" (at 4.445 0.33 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 10.795 0.33 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 16 "SENSE") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-218-3_Vertical" (layer "F.Cu")
    (at 170.18 114.3)
    (descr "TO-218-3, Vertical, RM 5.475mm, SOT-93, see https://www.vishay.com/docs/95214/fto218.pdf")
    (tags "TO-218-3 Vertical RM 5.475mm SOT-93")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 5.475 -4.29) (layer "F.SilkS"))
    (fp_text value "FDA59N30" (at 5.475 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.475 -4.29) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U1-Pad3)") (pinfunction "G") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 5.475 0) (size 3 3) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 23 "LINE") (pinfunction "D") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 10.95 0) (size 3 3) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 16 "SENSE") (pinfunction "S") (pintype "unspecified"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-218-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (at 102.87 118.11)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 7.75 7.75) (drill 3.8) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 111.76 119.36 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 4.425 0 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 10.775 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork" (layer "F.Cu")
    (at 175.655 129.54)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "LINE1" (at 7.225 4.445) (layer "F.SilkS"))
    (fp_text value "LINE" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.75 7.75) (drill 3.8) (layers "*.Cu" "*.Mask")
      (net 23 "LINE") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:KSA_Tactile_SPST" (layer "F.Cu")
    (at 157.48 106.68)
    (descr "KSA http://www.ckswitches.com/media/1457/ksa_ksl.pdf")
    (tags "SWITCH SMD KSA SW")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 2.54 -2) (layer "F.SilkS"))
    (fp_text value "Trip" (at 2.54 10) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 4) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 13 "TRIP") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 7.62) (size 1.778 1.778) (drill 1.143) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.54 7.62) (size 1.778 1.778) (drill 1.143) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 0 7.62) (size 1.778 1.778) (drill 1.143) (layers "*.Cu" "*.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/KSA_Tactile_SPST.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 137.16 120.65)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 4.445 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 10.795 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (at 102.87 67.31)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 7.75 7.75) (drill 3.8) (layers "*.Cu" "*.Mask")
      (clearance 1))
  )
  (footprint "Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork" (layer "F.Cu")
    (at 137.16 132.08)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "-PS1" (at 0 2.25) (layer "F.SilkS"))
    (fp_text value "Ground" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork" (layer "F.Cu")
    (at 175.655 68.58)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "LOAD1" (at 7.86 -3.81) (layer "F.SilkS"))
    (fp_text value "LOAD" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.75 7.75) (drill 3.8) (layers "*.Cu" "*.Mask")
      (net 24 "LOAD") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 129.54 66.02 -90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 10.815 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 4.465 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0 270) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 139.105 89.535)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 2.5 2.54) (layer "F.SilkS"))
    (fp_text value "1u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm_IRGrey" (layer "F.Cu")
    (at 152.4 86.36 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "Closed" (at 6.675 -2.54) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_IRGrey.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3266Y_Vertical" (layer "F.Cu")
    (at 116.845 73.66 90)
    (descr "Potentiometer, vertical, Bourns 3266Y, https://www.bourns.com/docs/Product-Datasheets/3266.pdf")
    (tags "Potentiometer vertical Bourns 3266Y")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV1" (at -2.54 -3.41 90) (layer "F.SilkS"))
    (fp_text value "Pickup adj." (at -2.54 3.59 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.15 0.09 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(R3-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(RV1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3266Y_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 180.015 106.68 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R_shunt1" (at 6.35 0.325 90) (layer "F.SilkS"))
    (fp_text value "1" (at 12.065 0.325 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 16 "SENSE") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (zone_connect 0) (thermal_bridge_width 1))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 137.16 127)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 4.445 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 10.795 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 13 "TRIP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 160.02 81.26 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R10" (at 4.425 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 10.775 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3266Y_Vertical" (layer "F.Cu")
    (at 121.92 114.3)
    (descr "Potentiometer, vertical, Bourns 3266Y, https://www.bourns.com/docs/Product-Datasheets/3266.pdf")
    (tags "Potentiometer vertical Bourns 3266Y")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV2" (at -2.92 -3.41) (layer "F.SilkS"))
    (fp_text value "Time Delay" (at -2.54 3.59) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.15 0.09) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(RV2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3266Y_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork" (layer "F.Cu")
    (at 142.24 132.08)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP0" (at 0 2.25) (layer "F.SilkS"))
    (fp_text value "Ground" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (zone_connect 2))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (at 191.77 130.81)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 7.75 7.75) (drill 3.8) (layers "*.Cu" "*.Mask")
      (clearance 1))
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 144.78 81.26 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R7" (at 4.425 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 10.775 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(R6-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm_IRGrey" (layer "F.Cu")
    (at 129.54 88.88 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 2.52 -3.96 90) (layer "F.SilkS"))
    (fp_text value "Pick-up" (at 1.27 3.96 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_IRGrey.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm_IRGrey" (layer "F.Cu")
    (at 160.02 86.36 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "Tripped" (at -3.81 -2.54) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D3-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_IRGrey.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 137.16 66.02 -90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 10.815 0 90) (layer "F.SilkS"))
    (fp_text value "4k7" (at 4.465 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0 270) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(R6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 109.855 88.9 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 10.795 -0.02 90) (layer "F.SilkS"))
    (fp_text value "47k" (at 4.445 -0.02 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.7mm_Pad" (layer "F.Cu")
    (at 191.77 67.31)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference " " (at 0 -4.7) (layer "F.SilkS"))
    (fp_text value " " (at 0 4.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7.75 7.75) (drill 3.8) (layers "*.Cu" "*.Mask")
      (clearance 1))
  )
  (footprint "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 125.73 114.26 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 4.26 -2.5 90) (layer "F.SilkS"))
    (fp_text value "0u1" (at 2.5 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (at 119.38 104.14)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(RV2-Pad2)") (pinfunction "Pin_1") (pintype "passive") (zone_connect 2))
  )
  (footprint "Button_Switch_THT:KSA_Tactile_SPST" (layer "F.Cu")
    (at 147.32 106.68)
    (descr "KSA http://www.ckswitches.com/media/1457/ksa_ksl.pdf")
    (tags "SWITCH SMD KSA SW")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 2.54 -2) (layer "F.SilkS"))
    (fp_text value "Close" (at 2.54 10) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 4) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(R1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 7.62) (size 1.778 1.778) (drill 1.143) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.54 7.62) (size 1.778 1.778) (drill 1.143) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 0 7.62) (size 1.778 1.778) (drill 1.143) (layers "*.Cu" "*.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/KSA_Tactile_SPST.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Axial_L17.0mm_D7.0mm_P25.00mm_Horizontal" (layer "F.Cu")
    (at 102.87 104.14 90)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=17*7.0mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 25mm  length 17mm diameter 7.0mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 7.42 0 90) (layer "F.SilkS"))
    (fp_text value "2u2" (at 17.58 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 12.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 25 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L17.0mm_D7.0mm_P25.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork" (layer "F.Cu")
    (at 129.54 132.08)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "+PS1" (at 0 2.25) (layer "F.SilkS"))
    (fp_text value "+9 Volts" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm_Socket" (layer "F.Cu")
    (at 147.32 100.32 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "4011" (at 3.81 17.78 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(R1-Pad2)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U1-Pad2)") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U1-Pad3)") (pintype "output"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U1-Pad2)") (pintype "output"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U1-Pad3)") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "TRIP") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U1-Pad2)") (pintype "input"))
    (pad "9" thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U1-Pad2)") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(U1-Pad10)") (pintype "output"))
    (pad "11" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D3-Pad1)") (pintype "output"))
    (pad "12" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(U1-Pad10)") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(U1-Pad10)") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown" (layer "F.Cu")
    (at 123.53 132.08 90)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 2.54 -20.58 90) (layer "F.SilkS"))
    (fp_text value "L7805" (at 2.54 2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -20.58 90) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 2.54 -16.66 90) (size 3.8 3.8) (drill 3.8) (layers "F&B.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.75 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pinfunction "IN") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.75 1.75) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.75 1.75) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 129.54 126.98 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R8" (at 4.425 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 10.775 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (layer "F.Cu")
    (at 152.4 66.04 -90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R9" (at 10.795 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 4.445 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pintype "passive"))
    (pad "2" thru_hole circle (at 15.24 0 270) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-218-3_Vertical" (layer "F.Cu")
    (at 170.185 84.53)
    (descr "TO-218-3, Vertical, RM 5.475mm, SOT-93, see https://www.vishay.com/docs/95214/fto218.pdf")
    (tags "TO-218-3 Vertical RM 5.475mm SOT-93")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 5.475 -4.29) (layer "F.SilkS"))
    (fp_text value "FDA59N30" (at 5.475 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.475 -4.29) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U1-Pad3)") (pinfunction "G") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 5.475 0) (size 3 3) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 24 "LOAD") (pinfunction "D") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 10.95 0) (size 3 3) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "S") (pintype "unspecified") (zone_connect 1) (thermal_bridge_width 1))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-218-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm_IRGrey" (layer "F.Cu")
    (at 130.81 104.12 -90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 1.27 4.445 90) (layer "F.SilkS"))
    (fp_text value "Low Batt" (at 1.27 3.96 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_IRGrey.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 116.84 83.86 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 -2.5 90) (layer "F.SilkS"))
    (fp_text value "1u" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 133.35 71.08 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 7.58 0 90) (layer "F.SilkS"))
    (fp_text value "1u" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm_Socket" (layer "F.Cu")
    (at 132.085 92.7 -90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "battgrid_breaker.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "LM339" (at 3.81 17.57 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(C1-Pad1)") (pintype "open_collector"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-Pad1)") (pintype "open_collector"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "+9V") (pinfunction "V+") (pintype "power_in"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(C3-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(RV1-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(RV1-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(C3-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "8" thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(C1-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "9" thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(RV2-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "-") (pintype "input"))
    (pad "11" thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(R6-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "13" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D2-Pad1)") (pintype "open_collector"))
    (pad "14" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "TRIP") (pintype "open_collector"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 96.52 60.96) (end 198.12 137.16)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Low 9V\nbattery" (at 137.16 105.41) (layer "F.SilkS"))
  (gr_text "Time delay\n  adjust" (at 118.745 107.95) (layer "F.SilkS"))
  (gr_text "Close" (at 149.86 116.84) (layer "F.SilkS"))
  (gr_text "Closed\n(red)" (at 145.415 85.805) (layer "F.SilkS"))
  (gr_text "Circuit breaker with\ndefinite-time, directional\novercurrent protection\n(C) 2022 Tony R. Kuphaldt" (at 158.75 132.08) (layer "F.SilkS"))
  (gr_text "(current out)" (at 175.895 62.23) (layer "F.SilkS"))
  (gr_text "Overcurrent sensing works only for current in the \ndirection of the arrow.  Current passing through the \ncircuit breaker in the opposite direction is unmonitored\nand will never cause the breaker to {dblquote}pick up{dblquote}" (at 191.135 99.695 90) (layer "F.SilkS"))
  (gr_text "(current in)" (at 175.895 135.89) (layer "F.SilkS"))
  (gr_text "Trip" (at 160.02 116.84) (layer "F.SilkS"))
  (gr_text "5-Volt\nregulator" (at 114.3 129.54) (layer "F.SilkS"))
  (gr_text "Tripped\n(green)" (at 164.465 85.725) (layer "F.SilkS"))
  (gr_text "Pickup\nadjust" (at 122.555 74.93) (layer "F.SilkS"))
  (gr_text "Pick-up" (at 135.89 86.36) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 197.485 136.525)
        (xy 97.155 136.525)
        (xy 97.155 61.595)
        (xy 197.485 61.595)
      )
    )
  )
)
