#   This is "instr.set", the main instruction set description file.

#   The format of this file is as follows.  First of all, blank lines
#   and lines whose first character is a '#' are comment lines.

#   Otherwise, each line consists of one or more fields, separated by
#   spaces (but not tabs).

#   The first field is the opcode field.  It looks like the following:
#       _^nxxx
#   or  _^nxxx/xxx
#   or  _^nxxx#xxx
#   or  _^nxxx*xxx
#   Here:
#    _   (if present) signifies that the line applies only to the
#        assembler.
#    ^n  (if present) is ^0 for AAD or AAM, ^1 for DB, ^2 for DW,
#        ^3 for DD, ^4 for ORG, and ^5 for 32 bit operand prefix.
#        ^6 a32, ^7 a16, ^8 o32, ^9 o16, ^10..^13: D/W mnemonic suffix:
#         ^10 controls operand size prefix 66h, optional
#         ^11 controls operand size prefix 66h, required
#         ^12 controls address size prefix 67h, optional
#         ^13 controls address size prefix 67h, required
#          (^13 is not currently supported)
#         ^14 Special mnemonic (AAD,AAM,DB,DW,DD,ORG,A32,A16,O32,O16)
#         ^15 Special mnemonic, specified by a byte (LOCK,REP,seg)
#    xxx is an op code mnemonic.
#    '/' mean that the following opcode is the 32-bit variant of the
#        first one, and a 66h prefix will switch.
#    '#' mean that the following opcode is the 32-bit variant of the
#        first one, and a 67h prefix will switch.
#    '*' mean that the preceding opcode occurs with a WAIT instruction;
#        the following, without.

#   The remaining fields describe the possible variants of the instruction.
#   They have the following formats:
#       _Lxx/r.;n
#       _Lxx/r*;n
#       _Lxx/r&;n
#       _DLxx/r:kk;n
#   Here:
#       _   (if present) means that this variant is to be used only by
#           the assembler.
#       D   (if present) means that this variant is to be used only by
#           the disassembler.
#       L   (if present) means that this is a lockable instruction.
#       xx  are one or two bytes of the instruction field. Note that if the
#           disassembler-only D and lockable L are both not present and the
#           opcode is to start with a digit 'D' (13 in hexadecimal) then the
#           digit has to be lowercase to not be misdetected.
#       /r  (if present) specifies the "r" part in a MOD MEM/REG byte.
#       .   indicates that the instruction has no operands.
#       *   indicates that the byte is a prefix (LOCK or REP...).
#       &   indicates that the byte is a segment prefix.
#       :kk gives an index into the file "instr.key".  That file gives
#           the operand list associated to the key.  The key consists of
#           two hex digits.
#       ;n  (if present) indicates the processor on which this
#           instruction first appeared.  Here n may be 1 through 6.
#
#   The order of the variants is important, because the assembler will take
#   the first one that fits the input line.

#   References:
#
#   Instruction set from the Intel Pentium Family User's Manual, Vol. 3:
#   Architecture and Programming Manual.  Information on earlier processors
#   from various Intel and third party documentation.  Information on new
#   Pentium Pro <TM> instructions from http://x86.metronet.com
#   (http://198.215.126.12).

#   History:
#   v1.09: - "loop" opcode has no "ecx" operand anymore in 32-bit.
#          - changed order 1 3 to 3 1 for arith opcodes.
#   v1.10: - "loopw", "loopzw" and "loopnzw" variants added.
#   v1.18: - "fldenvw", "fldenvd", "fstenvw", "fstenvd" variants added.
#          - "fsavew", "fsaved", "frstorw", "frstord" variants added.
#          - "movd" and "movq" added.
#   lDebug: retn, int3, int03, int1, int01, icebp
#           a32, a16, o32, o16, common D/W mnemonic suffix
#           enterw, enterd, leavew, leaved
#           MMX instruction set
#           boxcb

# Usage of the works is permitted provided that this
# instrument is retained with the works, so that any entity
# that uses the works is notified of this instrument.
#
# DISCLAIMER: THE WORKS ARE WITHOUT WARRANTY.


_^6a32
_^7a16
_^8o32
_^9o16

boxcb fe/7:3B		# DOSBox callbacks
aaa 37.
^0aad d5:27
^0aam d4:27
aas 3f.
adc L83/2:03 14:01 L80/2:02 L10:04 12:05
add L83/0:03 04:01 L80/0:02 L00:04 02:05
and L83/4:03 24:01 L80/4:02 L20:04 22:05
arpl 63:06;2
bound 62:63;1
bsf 0fbc:08;3
bsr 0fbd:08;3
^5bswap 0fc8:09;4
bt 0fa3:8A;3 0fba/4:8B;3
btc L0fbb:0A;3 L0fba/7:0B;3
btr L0fb3:0A;3 L0fba/6:0B;3
bts L0fab:0A;3 L0fba/5:0B;3
call e8:GC ff/2:GA ff/3:GE 9a:GD
cbw/cwde 98.
clc f8.
cld fc.
cli fa.
clts 0f06.;2
cmc f5.
cmova 0f47:08;6
cmovae 0f43:08;6
cmovb 0f42:08;6
cmovbe 0f46:08;6
_cmovc 0f42:08;6
_cmove 0f44:08;6
cmovg 0f4f:08;6
cmovge 0f4d:08;6
cmovl 0f4c:08;6
cmovle 0f4e:08;6
_cmovna 0f46:08;6
_cmovnae 0f42:08;6
_cmovnb 0f43:08;6
_cmovnbe 0f47:08;6
_cmovnc 0f43:08;6
_cmovne 0f45:08;6
_cmovng 0f4e:08;6
_cmovnge 0f4c:08;6
_cmovnl 0f4d:08;6
_cmovnle 0f4f:08;6
cmovno 0f41:08;6
_cmovnp 0f4b:08;6
cmovns 0f49:08;6
cmovnz 0f45:08;6
cmovo 0f40:08;6
_cmovp 0f4a:08;6
cmovpe 0f4a:08;6
cmovpo 0f4b:08;6
cmovs 0f48:08;6
cmovz 0f44:08;6
cmp 83/7:83 3c:01 80/7:82 38:84 3a:05
cmpsb a6.
^11cmps a7.
cmpxchg L0fb0:04;4
cmpxchg8b 0fc7/1:0F;5
cpuid 0fa2.;5
cwd/cdq 99.
daa 27.
das 2f.
_^1db
_^3dd
dec 48:11 Lfe/1:10 DLff/1:10
div f6/6:90
_^2dw
emms 0f77.;5
^10enter c8:12;1
f2xm1 d9f0.
fabs d9e1.
fadd d8/0:93 dc/0:94 d8c0:15 dcc0:16
faddp dec0:17 _dec1.
fiadd da/0:98 de/0:99
fbld df/4:9A
fbstp df/6:DA
fchs d9e0.
fclex*fnclex dbe2.
_fcmova dbd0:15;6
_fcmovae dbc0:15;6
fcmovb dac0:15;6
fcmovbe dad0:15;6
fcmove dac8:15;6
_fcmovna dad0:15;6
_fcmovnae dac0:15;6
fcmovnb dbc0:15;6
fcmovnbe dbd0:15;6
fcmovne dbc8:15;6
fcmovnu dbd8:15;6
_fcmovnz dbc8:15;6
fcmovu dad8:15;6
_fcmovz dac8:15;6
fcom d8/2:93 dc/2:94 d8d0:1C _d8d1.
fcomi dbf0:1C;6 _dbf1.;6
fcomip dff0:1C;6 _dff1.;6
fcomp d8/3:93 dc/3:94 d8d8:1C _d8d9.
fcompp ded9.
fcos d9ff.;3
fdecstp d9f6.
fdisi*fndisi dbe1.
fdiv d8/6:93 dc/6:94 d8f0:15 dcf8:16
fdivp def8:17 _def9.
fidiv da/6:98 de/6:99
fdivr d8/7:93 dc/7:94 d8f8:15 dcf0:16
fdivrp def0:17 _def1.
fidivr da/7:98 de/7:99
feni*fneni dbe0.
ffree ddc0:1B
ficom da/2:98 de/2:99
ficomp da/3:98 de/3:99
fild db/0:98 df/0:99 df/5:8F
fincstp d9f7.
finit*fninit dbe3.
fist db/2:D8 df/2:D9
fistp db/3:D8 df/3:D9 df/7:CF
fld d9/0:93 dd/0:94 db/5:9D d9c0:1B
fld1 d9e8.
fldl2t d9e9.
fldl2e d9ea.
fldpi d9eb.
fldlg2 d9ec.
fldln2 d9ed.
fldz d9ee.
fldcw*fnldcw d9/5:99
^10fldenv d9/4:9E
fmul d8/1:93 dc/1:94 d8c8:15 dcc8:16
fmulp dec8:17 _dec9.
fimul da/1:98 de/1:99
fnop d9d0.
fpatan d9f3.
fprem d9f8.
fprem1 d9f5.;3
fptan d9f2.
frndint d9fc.
^10frstor dd/4:9E
^10fsave*fnsave dd/6:DE
fscale d9fd.
fsetpm*fnsetpm dbe4.;2
fsin d9fe.;3
fsincos d9fb.;3
fsqrt d9fa.
fst d9/2:D3 dd/2:D4 ddd0:1B
fstp d9/3:D3 dd/3:D4 db/7:DD ddd8:1B
fstcw*fnstcw d9/7:D9
^10fstenv*fnstenv d9/6:DE
fstsw*fnstsw dfe0:1F dd/7:D9
fsub d8/4:93 dc/4:94 d8e0:15 dce8:16
fsubp dee8:17 _dee9.
fisub da/4:98 de/4:99
fsubr d8/5:93 dc/5:94 d8e8:15 dce0:16
fsubrp dee0:17 _dee1.
fisubr da/5:98 de/5:99
ftst d9e4.
fucom dde0:1C;3 _dde1.;3
fucomi dbe8:1C;6 _dbe9.;6
fucomip dfe8:1C;6 _dfe9.;6
fucomp dde8:1C;3 _dde9.;3
fucompp dae9.;3
_fwait 9b.
fxam d9e5.
fxch d9c8:1C _d9c9.
fxtract d9f4.
fyl2x d9f1.
fyl2xp1 d9f9.
hlt f4.
idiv f6/7:90
imul f6/5:90 0faf:08;3 6b:20;1 _6b:21;1 69:22;1 _69:23;1
in e4:24 ec:25
inc 40:11 Lfe/0:10 DLff/0:10
insb 6c.;1
^11ins 6d.;1
int _cc:26 cd:64
int1 f1:G9;6
_int01 f1:G9;6
_icebp f1:G9;6
int3 cc:G9
_int03 cc:G9
into ce:G9
invd 0f08.;4
invlpg 0f01/7:1E;4
^10iret cf:G9
ja 77:28 0f87:0C;3
jae 73:28 0f83:0C;3
jb 72:28 0f82:0C;3
jbe 76:28 0f86:0C;3
_jc 72:28 0f82:0C;3
jcxz#jecxz e3:28
_je 74:28 0f84:0C;3
jg 7f:28 0f8f:0C;3
jge 7d:28 0f8d:0C;3
jl 7c:28 0f8c:0C;3
jle 7e:28 0f8e:0C;3
_jna 76:28 0f86:0C;3
_jnae 72:28 0f82:0C;3
_jnb 73:28 0f83:0C;3
_jnbe 77:28 0f87:0C;3
_jnc 73:28 0f83:0C;3
_jne 75:28 0f85:0C;3
_jng 7e:28 0f8e:0C;3
_jnge 7c:28 0f8c:0C;3
_jnl 7d:28 0f8d:0C;3
_jnle 7f:28 0f8f:0C;3
jno 71:28 0f81:0C;3
_jnp 7b:28 0f8b:0C;3
jns 79:28 0f89:0C;3
jnz 75:28 0f85:0C;3
jo 70:28 0f80:0C;3
_jp 7a:28 0f8a:0C;3
jpe 7a:28 0f8a:0C;3
jpo 7b:28 0f8b:0C;3
js 78:28 0f88:0C;3
jz 74:28 0f84:0C;3
jmp eb:28 e9:0C ff/4:62 ff/5:0E ea:0D
lahf 9f.
lar 0f02:08;2
lds c5:07
lss 0fb2:07;3
les c4:07
lfs 0fb4:07;3
lgs 0fb5:07;3
lea 8d:60
^10leave c9:G9;1
lgdt 0f01/2:9E;2
lidt 0f01/3:9E;2
lldt 0f00/2:AA;2
lmsw 0f01/6:AA;2
#lock f0*
^15lock f0
lodsb ac.
^11lods ad.
^12loop e2:28
^12loopz e1:28
_^12loope e1:28
^12loopnz e0:28
_^12loopne e0:28
# The _loopxx entries have an oplist 28 variant because
#  the assembler finds these mnemonics before the ASA
#  mnemonics. However, if all oplists of a mnemonic are
#  failed, the assembler doesn't next search for another
#  mnemonic match but considers the instruction invalid.
# Therefore without an asize suffix we find the _loopxx
#  mnemonic and either match rel8, e_cx or just rel8.
#  Only when the asize suffix is present the normal
#  loopxx mnemonics are found and used. The disassembler
#  is not affected, it always uses the ASA mnemonics.
_loop e2:65 e2:28
_loopz e1:65 e1:28
_loope e1:65 e1:28
_loopnz e0:65 e0:28
_loopne e0:65 e0:28
lsl 0f03:08;2
ltr 0f00/3:AA;2
# F=mov a,[mem], G=mov [mem],a  4=mov a,r
mov a0:2D a2:2E 88:C4 8a:05 8c:2B 8e:2C b0:2F b8:30 c6/0:C2 0f20:47;3 0f22:48;3 0f21:49;3 0f23:4A;3 0f24:4B;3 0f26:4C;3

# MMX instruction set (excluding emms)
movd 0f6e:4D;5 0f7e:4E;5
#movntq 0fe7:53;5		#SSE
movq 0f6f:4F;5 0f7f:50;5
#maskmovq 0ff7:58;5		#SSE
packssdw 0f6b:4F;5
packsswb 0f63:4F;5
packuswb 0f67:4F;5
paddb 0ffc:4F;5
paddw 0ffd:4F;5
paddd 0ffe:4F;5
#paddq 0fd4:4F;5		#not MMX or SSE
paddsb 0fec:4F;5
paddsw 0fed:4F;5
paddusb 0fdc:4F;5
paddusw 0fdd:4F;5
pand 0fdb:4F;5
pandn 0fdf:4F;5
#pavgb 0fe0:4F;5		#SSE
#pavgw 0fe3:4F;5		#SSE
pcmpeqb 0f74:4F;5
pcmpeqw 0f75:4F;5
pcmpeqd 0f76:4F;5
pcmpgtb 0f64:4F;5		#pcmpgtpb ?
pcmpgtw 0f65:4F;5		#pcmpgtpw ?
pcmpgtd 0f66:4F;5		#pcmpgtpd ?
#pextrw 0fc5:54;5		#SSE
#pinsrw 0fc4:55;5 _0fc4:59;5	#SSE
pmaddwd 0ff5:4F;5
#pmaxsw 0fee:4F;5		#SSE
#pmaxub 0fde:4F;5		#SSE
#pminsw 0fea:4F;5		#SSE
#pminub 0fda:4F;5		#SSE
#pmovmskb 0fd7:56;5		#SSE
#pmulhuw 0fe4:4F;5		#SSE
pmulhw 0fe5:4F;5
pmullw 0fd5:4F;5
por 0feb:4F;5
#psadbw 0ff6:4F;5		#SSE
#pshufw 0f70:57;5		#SSE
psllw 0ff1:4F;5 0f71/6:52;5
pslld 0ff2:4F;5 0f72/6:52;5
psllq 0ff3:4F;5 0f73/6:52;5
psraw 0fe1:4F;5 0f71/4:52;5
psrad 0fe2:4F;5 0f72/4:52;5
psrlw 0fd1:4F;5 0f71/2:52;5
psrld 0fd2:4F;5 0f72/2:52;5
psrlq 0fd3:4F;5 0f73/2:52;5
psubb 0ff8:4F;5
psubw 0ff9:4F;5
psubd 0ffa:4F;5
#psubq 0ffb:4F;5		#not MMX or SSE
psubsb 0fe8:4F;5
psubsw 0fe9:4F;5
psubusb 0fd8:4F;5
psubusw 0fd9:4F;5
punpckhbw 0f68:4F;5
punpckhwd 0f69:4F;5
punpckhdq 0f6a:4F;5
punpcklbw 0f60:4F;5
punpcklwd 0f61:4F;5
punpckldq 0f62:4F;5
pxor 0fef:4F;5
##

movsb a4.
^11movs a5.
movsx 0fbe:31;3 0fbf:32;3
movzx 0fb6:31;3 0fb7:32;3
mul f6/4:90
neg Lf6/3:10
nop 90.
not Lf6/2:10
or L83/1:03 0c:01 L80/1:02 L08:04 0a:05
_^4org
out e6:33 ee:34
outsb 6e.;1
^11outs 6f.;1
pop 58:G1 8f/0:35 1f:Z4 07:Z1 17:Z3 0fa1:Z5;3 0fa9:Z6;3
^10popa 61:G9;1
^10popf 9d:G2
push 50:F1 ff/6:A9 _6a:37;1 _68:36;1 0e:S2 16:S3 1e:S4 06:S1 0fa0:S5;3 0fa8:S6;3
^10push 6a:37;1 68:36;1
^10pusha 60:G9;1
^10pushf 9c:G3
rcl d0/2:38 d2/2:39 c0/2:3A;1
rcr d0/3:38 d2/3:39 c0/3:3A;1
rol d0/0:38 d2/0:39 c0/0:3A;1
ror d0/1:38 d2/1:39 c0/1:3A;1
rdmsr 0f32.;5
rdtsc 0f31.;5
#rep f3*
#repe f3*
#repne f2*
^15rep f3
_^15repz f3
_^15repnz f2
^15repe f3
^15repne f2
^10retn c3:G2 c2:G7
_^10ret c3:G2 c2:G7
^10retf cb:G9 ca:G8
rsm 0faa.;5
sahf 9e.
_sal d0/4:38 d2/4:39 c0/4:3A;1
sar d0/7:38 d2/7:39 c0/7:3A;1
seg _26:41 _2e:42 _36:43 _3e:44 _64:45 _65:46
#es _26&
#cs _2e&
#ss _36&
#ds _3e&
#fs _64&
#gs _65&
^15es _26
^15cs _2e
^15ss _36
^15ds _3e
^15fs _64
^15gs _65
shl d0/4:38 d2/4:39 c0/4:3A;1 Dd0/6:38 Dd2/6:39 Dc0/6:3A;1
shr d0/5:38 d2/5:39 c0/5:3A;1
sbb L83/3:03 1c:01 L80/3:02 L18:04 1a:05
scasb ae.
^11scas af.
seta 0f97:3C;3
setae 0f93:3C;3
setb 0f92:3C;3
setbe 0f96:3C;3
_setc 0f92:3C;3
_sete 0f94:3C;3
setg 0f9f:3C;3
setge 0f9d:3C;3
setl 0f9c:3C;3
setle 0f9e:3C;3
_setna 0f96:3C;3
_setnae 0f92:3C;3
_setnb 0f93:3C;3
_setnbe 0f97:3C;3
_setnc 0f93:3C;3
_setne 0f95:3C;3
_setng 0f9e:3C;3
_setnge 0f9c:3C;3
_setnl 0f9d:3C;3
_setnle 0f9f:3C;3
setno 0f91:3C;3
_setnp 0f9b:3C;3
setns 0f99:3C;3
setnz 0f95:3C;3
seto 0f90:3C;3
_setp 0f9a:3C;3
setpe 0f9a:3C;3
setpo 0f9b:3C;3
sets 0f98:3C;3
setz 0f94:3C;3
sgdt 0f01/0:DE;2
sidt 0f01/1:DE;2
shld 0fa4:3D;3 0fa5:3E;3
shrd 0fac:3D;3 0fad:3E;3
sldt 0f00/0:E9;2
smsw 0f01/4:E9;2
stc f9.
std fd.
sti fb.
stosb aa.
^11stos ab.
str 0f00/1:EA;2
sub L83/5:03 2c:01 L80/5:02 L28:04 2a:05
_salc d6.;2
setalc d6.;2
test a8:01 f6/0:82 Df6/1:82 84:84 _84:05
ud0 0fff.;1
ud1 0fb9.;1
ud2 0f0b.;1
verr 0f00/4:AA;2
verw 0f00/5:AA;2
wait 9b.
wbinvd 0f09.;4
wrmsr 0f30.;5
xadd L0fc0:04;4
xchg 90:3F _90:40 _L86:04 L86:85
_xlat d7.
xlatb d7.
xor L83/6:03 34:01 L80/6:02 L30:04 32:05
